#define MICROPY_HW_BOARD_NAME "BLOK"
USB_PRODUCT = "BLOK"
    uint32_t THI = (*(uint32_t *)FUSES_HOT_TEMP_VAL_INT_ADDR & FUSES_HOT_TEMP_VAL_INT_Msk) >> FUSES_HOT_TEMP_VAL_INT_Pos;
    float TH = THI + convert_dec_to_frac(THD);
print(binascii.b2a_base64(b"fo"))
        # again, neither will "there" or "wither", since they have "the"
i1Qb$TE"rl
