<?xml version="1.0" encoding="UTF-8"?>

<package schemaVersion="1.3" xmlns:xs="http://www.w3.org/2001/XMLSchema-instance" xs:noNamespaceSchemaLocation="PACK.xsd">
  <name>CMSIS</name>
  <description>CMSIS (Cortex Microcontroller Software Interface Standard)</description>
  <vendor>ARM</vendor>
  <!-- <license>CMSIS\CMSIS_END_USER_LICENCE_AGREEMENT.rtf</license> -->
  <url>http://www.keil.com/pack/</url>

  <taxonomy>
    <description Cclass="Board Support">Generic Interfaces for Evaluation and Development Boards</description>
    <description Cclass="CMSIS" doc="CMSIS\Documentation\General\html\index.html">Cortex Microcontroller Software Interface Components</description>
    <description Cclass="Device" doc="CMSIS\Documentation\Core\html\index.html">Startup, System Setup</description>
    <description Cclass="CMSIS Driver" doc="CMSIS\Documentation\Driver\html\index.html">Unified Device Drivers compliant to CMSIS-Driver Specifications</description>
    <description Cclass="File System">File Drive Support and File System</description>
    <description Cclass="Graphics">Graphical User Interface</description>
    <description Cclass="Network">Network Stack using Internet Protocols</description>
    <description Cclass="USB">Universal Serial Bus Stack</description>
  </taxonomy>

  <releases>
    <release version="4.2.0" date="2014-09-24">
      Adding Cortex-M7 support
      - CMSIS-Core     4.00  (Cortex-M7 support, corrected C++ include guards in core header files)
      - CMSIS-DSP      1.4.4 (Cortex-M7 support and corrected out of bound issues)
      - CMSIS-PACK     1.3.1 (Cortex-M7 updates, clarification, corrected batch files in Tutorial)
      - CMSIS-SVD      1.2   (Cortex-M7 extensions)
      - CMSIS-RTOS RTX 4.75  (see revision history for details)
    </release>
    <release version="4.1.1" date="2014-06-30">
      - fixed conditions preventing the inclusion of the DSP library in projects for Infineon XMC4000 series devices
    </release>
    <release version="4.1.0" date="2014-06-12">
      - CMSIS-Driver   2.02  (incompatible update)
      - CMSIS-Pack     1.3   (see revision history for details)
      - CMSIS-DSP      1.4.2 (unchanged)
      - CMSIS-Core     3.30  (unchanged)
      - CMSIS-RTOS RTX 4.74  (unchanged)
      - CMSIS-RTOS API 1.02  (unchanged)
      - CMSIS-SVD      1.10  (unchanged)
      PACK:
      - removed G++ specific files from PACK
      - added Component Startup variant "C Startup"
      - added Pack Checking Utility 
      - updated conditions to reflect tool-chain dependency
      - added Taxonomy for Graphics
      - updated Taxonomy for unified drivers from "Drivers" to "CMSIS Drivers"
    </release>
    <release version="4.0.0">
      - CMSIS-Driver   2.00  Preliminary (incompatible update)
      - CMSIS-Pack     1.1   Preliminary
      - CMSIS-DSP      1.4.2 (see revision history for details)
      - CMSIS-Core     3.30  (see revision history for details)
      - CMSIS-RTOS RTX 4.74  (see revision history for details)
      - CMSIS-RTOS API 1.02  (unchanged)
      - CMSIS-SVD      1.10  (unchanged)
    </release>
    <release version="3.20.4">
      - CMSIS-RTOS 4.74 (see revision history for details)
      - PACK Extensions (Boards, Device Features, Flash Programming, Generators, Configuration Wizard). Schema version 1.1.
    </release>
    <release version="3.20.3">
      - CMSIS-Driver API Version 1.10 ARM prefix added (incompatible change)
      - CMSIS-RTOS 4.73 (see revision history for details)
    </release>
    <release version="3.20.2">
      - CMSIS-Pack documentation has been added
      - CMSIS-Drivers header and documentation have been added to PACK
      - CMSIS-CORE, CMSIS-DSP, CMSIS-RTOS API and CMSIS-SVD remain unchanged
    </release>
    <release version="3.20.1">
      - CMSIS-RTOS Keil RTX V4.72 has been added to PACK
      - CMSIS-CORE, CMSIS-DSP, CMSIS-RTOS API and CMSIS-SVD remain unchanged
    </release>
    <release version="3.20.0">
      The software portions that are deployed in the application program are now under a BSD license which allows usage
      of CMSIS components in any commercial or open source projects.  The Pack Description file Arm.CMSIS.pdsc describes the use cases
      The individual components have been update as listed below:
      - CMSIS-CORE adds functions for setting breakpoints, supports the latest GCC Compiler, and contains several corrections.
      - CMSIS-DSP library is optimized for more performance and contains several bug fixes.
      - CMSIS-RTOS API is extended with capabilities for short timeouts, Kernel initialization, and prepared for a C++ interface.
      - CMSIS-SVD is unchanged.
    </release>
  </releases>

  <devices>
    <!-- ******************************  Cortex-M0  ****************************** -->
    <family Dfamily="ARM Cortex M0" Dvendor="ARM:82">
      <book      name="Device\ARM\Documents\cortex_m0_dgug.pdf"       title="Cortex-M4 Device Generic Users Guide"/>
      <description>
The Cortex-M0 processor is an entry-level 32-bit ARM Cortex processor designed
for a broad range of embedded applications. It offers significant benefits to developers,
including:
- simple, easy-to-use programmers model
- highly efficient ultra-low power operation
- excellent code density
- deterministic, high-performance interrupt handling
- upward compatibility with the rest of the Cortex-M processor family.
      </description>
      <debug     svd="Device\ARM\SVD\ARMCM0.svd"/>
      <memory    id="IROM1"                                 start="0x00000000"  size="0x40000"  startup="1"   default="1"/>
      <memory    id="IRAM1"                                 start="0x20000000"  size="0x20000"  init   ="0"   default="1"/>
      <algorithm name="Device\ARM\Flash\NEW_DEVICE.FLM"     start="0x00000000"  size="0x40000"  default="1"/>

      <device Dname="ARMCM0">
        <processor Dcore="Cortex-M0" DcoreVersion="r0p0" Dfpu="0" Dmpu="0" Dendian="Configurable" Dclock="10000000"/>
        <compile   header="Device\ARM\ARMCM0\Include\ARMCM0.h"    define="ARMCM0"/>
      </device>
    </family>

    <!-- ******************************  Cortex-M0P  ****************************** -->
    <family Dfamily="ARM Cortex M0 plus" Dvendor="ARM:82">
      <book      name="Device\ARM\Documents\cortex_m0p_dgug.pdf"       title="Cortex-M4 Device Generic Users Guide"/>
      <description>
The Cortex-M0+ processor is an entry-level 32-bit ARM Cortex processor designed
for a broad range of embedded applications. It offers significant benefits to developers,
including:
- simple, easy-to-use programmers model
- highly efficient ultra-low power operation
- excellent code density
- deterministic, high-performance interrupt handling
- upward compatibility with the rest of the Cortex-M processor family.
      </description>
      <debug     svd="Device\ARM\SVD\ARMCM0P.svd"/>
      <memory    id="IROM1"                                 start="0x00000000"  size="0x40000"  startup="1"   default="1"/>
      <memory    id="IRAM1"                                 start="0x20000000"  size="0x20000"  init   ="0"   default="1"/>
      <algorithm name="Device\ARM\Flash\NEW_DEVICE.FLM"     start="0x00000000"  size="0x40000"  default="1"/>

      <device Dname="ARMCM0P">
        <processor Dcore="Cortex-M0+" DcoreVersion="r0p1" Dfpu="0" Dmpu="0" Dendian="Configurable" Dclock="10000000"/>
        <compile   header="Device\ARM\ARMCM0plus\Include\ARMCM0plus.h"  define="ARMCM0P"/>
      </device>
    </family>

    <!-- ******************************  Cortex-M3  ****************************** -->
    <family Dfamily="ARM Cortex M3" Dvendor="ARM:82">
      <book      name="Device\ARM\Documents\cortex_m3_dgug.pdf"       title="Cortex-M3 Device Generic Users Guide"/>
      <description>
The Cortex-M3 processor is an entry-level 32-bit ARM Cortex processor designed
for a broad range of embedded applications. It offers significant benefits to developers,
including:
- simple, easy-to-use programmers model
- highly efficient ultra-low power operation
- excellent code density
- deterministic, high-performance interrupt handling
- upward compatibility with the rest of the Cortex-M processor family.
      </description>
      <debug     svd="Device\ARM\SVD\ARMCM3.svd"/>
      <memory    id="IROM1"                                 start="0x00000000"  size="0x40000"  startup="1"   default="1"/>
      <memory    id="IRAM1"                                 start="0x20000000"  size="0x20000"  init   ="0"   default="1"/>
      <algorithm name="Device\ARM\Flash\NEW_DEVICE.FLM"     start="0x00000000"  size="0x40000"  default="1"/>

      <device Dname="ARMCM3">
        <processor Dcore="Cortex-M3" DcoreVersion="r2p1" Dfpu="0" Dmpu="1" Dendian="Configurable" Dclock="10000000"/>
        <compile   header="Device\ARM\ARMCM3\Include\ARMCM3.h"    define="ARMCM3"/>
      </device>
    </family>

    <!-- ******************************  Cortex-M4  ****************************** -->
    <family Dfamily="ARM Cortex M4" Dvendor="ARM:82">
      <book      name="Device\ARM\Documents\cortex_m4_dgug.pdf"       title="Cortex-M4 Device Generic Users Guide"/>
      <description>
The Cortex-M4 processor is an entry-level 32-bit ARM Cortex processor designed
for a broad range of embedded applications. It offers significant benefits to developers,
including:
- simple, easy-to-use programmers model
- highly efficient ultra-low power operation
- excellent code density
- deterministic, high-performance interrupt handling
- upward compatibility with the rest of the Cortex-M processor family.
      </description>
      <debug     svd="Device\ARM\SVD\ARMCM4.svd"/>
      <memory    id="IROM1"                                 start="0x00000000"  size="0x80000"  startup="1"   default="1"/>
      <memory    id="IRAM1"                                 start="0x20000000"  size="0x20000"  init   ="0"   default="1"/>
      <algorithm name="Device\ARM\Flash\NEW_DEVICE.FLM"     start="0x00000000"  size="0x80000"  default="1"/>

      <device Dname="ARMCM4">
        <processor Dcore="Cortex-M4" DcoreVersion="r0p1" Dfpu="0" Dmpu="1" Dendian="Configurable" Dclock="10000000"/>
        <compile   header="Device\ARM\ARMCM4\Include\ARMCM4.h"    define="ARMCM4"/>
      </device>

      <device Dname="ARMCM4_FP">
        <processor Dcore="Cortex-M4" DcoreVersion="r0p1" Dfpu="1" Dmpu="1" Dendian="Configurable" Dclock="10000000"/>
        <compile   header="Device\ARM\ARMCM4\Include\ARMCM4_FP.h" define="ARMCM4_FP"/>
      </device>
    </family>

    <!-- ******************************  Cortex-M7  ****************************** -->
    <family Dfamily="ARM Cortex M7" Dvendor="ARM:82">
      <!-- <book      name="Documents\..."                 title="ARM Cortex-M4 Device Generic Users Guide"/> -->
      <description>
The Cortex-M4 processor is an entry-level 32-bit ARM Cortex processor designed
for a broad range of embedded applications. It offers significant benefits to developers,
including:
- simple, easy-to-use programmers model
- highly efficient ultra-low power operation
- excellent code density
- deterministic, high-performance interrupt handling
- upward compatibility with the rest of the Cortex-M processor family.
      </description>
      <debug     svd="Device\ARM\SVD\ARMCM7.svd"/>
      <memory    id="IROM1"                                 start="0x00000000"  size="0x80000"  startup="1"   default="1"/>
      <memory    id="IRAM1"                                 start="0x20000000"  size="0x20000"  init   ="0"   default="1"/>
      <algorithm name="Device\ARM\Flash\NEW_DEVICE.FLM"     start="0x00000000"  size="0x80000"  default="1"/>

      <device Dname="ARMCM7">
        <processor Dcore="Cortex-M7" DcoreVersion="r0p0" Dfpu="0" Dmpu="1" Dendian="Configurable" Dclock="10000000"/>
        <compile   header="Device\ARM\ARMCM7\Include\ARMCM7.h"    define="ARMCM7"/>
      </device>

      <device Dname="ARMCM7_SP">
        <processor Dcore="Cortex-M7" DcoreVersion="r0p0" Dfpu="SP_FPU" Dmpu="1" Dendian="Configurable" Dclock="10000000"/>
        <compile   header="Device\ARM\ARMCM7\Include\ARMCM7_SP.h" define="ARMCM7_SP"/>
      </device>

      <device Dname="ARMCM7_DP">
        <processor Dcore="Cortex-M7" DcoreVersion="r0p0" Dfpu="DP_FPU" Dmpu="1" Dendian="Configurable" Dclock="10000000"/>
        <compile   header="Device\ARM\ARMCM7\Include\ARMCM7_DP.h" define="ARMCM7_DP"/>
      </device>
    </family>

    <!-- ******************************  ARMSC000  ****************************** -->
    <family Dfamily="ARM SC000" Dvendor="ARM:82">
      <description>
The ARM SC000 processor is an entry-level 32-bit ARM Cortex processor designed
for a broad range of secure embedded applications. It offers significant benefits to developers,
including:
- simple, easy-to-use programmers model
- highly efficient ultra-low power operation
- excellent code density
- deterministic, high-performance interrupt handling
      </description>
      <debug     svd="Device\ARM\SVD\ARMSC000.svd"/>
      <memory    id="IROM1"                                 start="0x00000000"  size="0x40000"  startup="1"   default="1"/>
      <memory    id="IRAM1"                                 start="0x20000000"  size="0x20000"  init   ="0"   default="1"/>
      <algorithm name="Device\ARM\Flash\NEW_DEVICE.FLM"     start="0x00000000"  size="0x40000"  default="1"/>

      <device Dname="ARMSC000">
        <processor Dcore="SC000" DcoreVersion="r0p1" Dfpu="0" Dmpu="0" Dendian="Configurable" Dclock="10000000"/>
        <compile   header="Device\ARM\ARMSC000\Include\ARMSC000.h" define="ARMSC000"/>
      </device>
    </family>


    <!-- ******************************  ARMSC300  ****************************** -->
    <family Dfamily="ARM SC300" Dvendor="ARM:82">
      <description>
The ARM SC300 processor is an entry-level 32-bit ARM Cortex processor designed
for a broad range of secure embedded applications. It offers significant benefits to developers,
including:
- simple, easy-to-use programmers model
- highly efficient ultra-low power operation
- excellent code density
- deterministic, high-performance interrupt handling
      </description>
      <debug     svd="Device\ARM\SVD\ARMSC300.svd"/>
      <memory    id="IROM1"                                 start="0x00000000"  size="0x40000"  startup="1"   default="1"/>
      <memory    id="IRAM1"                                 start="0x20000000"  size="0x20000"  init   ="0"   default="1"/>
      <algorithm name="Device\ARM\Flash\NEW_DEVICE.FLM"     start="0x00000000"  size="0x40000"  default="1"/>

      <device Dname="ARMSC300">
        <processor Dcore="SC300" DcoreVersion="r0p1" Dfpu="0" Dmpu="0" Dendian="Configurable" Dclock="10000000"/>
        <compile   header="Device\ARM\ARMSC300\Include\ARMSC300.h" define="ARMSC300"/>
      </device>
    </family>

  </devices>


  <apis>
    <!-- CMSIS-RTOS API -->
    <api Cclass="CMSIS" Cgroup="RTOS" Capiversion="1.0" exclusive="1">
      <description>CMSIS-RTOS API for Cortex-M, SC000, and SC300</description>
      <files>
        <file category="doc" name="CMSIS\Documentation\RTOS\html\index.html"/>
      </files>
    </api>
    <api Cclass="CMSIS Driver" Cgroup="USART" Capiversion="2.01" exclusive="0">
        <description>USART Driver API for Cortex-M</description>
        <files>
          <file category="doc" name="CMSIS\Documentation\Driver\html\group__usart__interface__gr.html" />
          <file category="header" name="CMSIS\Driver\Include\Driver_USART.h" />
        </files>
      </api>
    <api Cclass="CMSIS Driver" Cgroup="SPI" Capiversion="2.01" exclusive="0">
        <description>SPI Driver API for Cortex-M</description>
        <files>
          <file category="doc" name="CMSIS\Documentation\Driver\html\group__spi__interface__gr.html" />
          <file category="header" name="CMSIS\Driver\Include\Driver_SPI.h" />
        </files>
      </api>
      <api Cclass="CMSIS Driver" Cgroup="I2C" Capiversion="2.02" exclusive="0">
        <description>I2C Driver API for Cortex-M</description>
        <files>
          <file category="doc" name="CMSIS\Documentation\Driver\html\group__i2c__interface__gr.html"/>
          <file category="header" name="CMSIS\Driver\Include\Driver_I2C.h" />
        </files>
      </api>
    <api Cclass="CMSIS Driver" Cgroup="Flash" Capiversion="2.00" exclusive="0">
        <description>Flash Driver API for Cortex-M</description>
        <files>
          <file category="doc" name="CMSIS\Documentation\Driver\html\group__flash__interface__gr.html" />
          <file category="header" name="CMSIS\Driver\Include\Driver_Flash.h" />
        </files>
      </api>
      <api Cclass="CMSIS Driver" Cgroup="MCI" Capiversion="2.02" exclusive="0">
        <description>MCI Driver API for Cortex-M</description>
        <files>
          <file category="doc" name="CMSIS\Documentation\Driver\html\group__mci__interface__gr.html" />
          <file category="header" name="CMSIS\Driver\Include\Driver_MCI.h" />
        </files>
      </api>
    <api Cclass="CMSIS Driver" Cgroup="NAND" Capiversion="2.01" exclusive="0">
        <description>NAND Flash Driver API for Cortex-M</description>
        <files>
          <file category="doc" name="CMSIS\Documentation\Driver\html\group__nand__interface__gr.html" />
          <file category="header" name="CMSIS\Driver\Include\Driver_NAND.h" />
        </files>
      </api>
    <api Cclass="CMSIS Driver" Cgroup="Ethernet" Capiversion="2.01" exclusive="0">
        <description>Ethernet MAC and PHY Driver API for Cortex-M</description>
        <files>
          <file category="doc" name="CMSIS\Documentation\Driver\html\group__eth__interface__gr.html" />
          <file category="header" name="CMSIS\Driver\Include\Driver_ETH_MAC.h" />
          <file category="header" name="CMSIS\Driver\Include\Driver_ETH_PHY.h" />
        </files>
      </api>
    <api Cclass="CMSIS Driver" Cgroup="Ethernet MAC" Capiversion="2.01" exclusive="0">
        <description>Ethernet MAC Driver API for Cortex-M</description>
        <files>
          <file category="doc" name="CMSIS\Documentation\Driver\html\group__eth__mac__interface__gr.html" />
          <file category="header" name="CMSIS\Driver\Include\Driver_ETH_MAC.h" />
        </files>
      </api>
    <api Cclass="CMSIS Driver" Cgroup="Ethernet PHY" Capiversion="2.00" exclusive="0">
        <description>Ethernet PHY Driver API for Cortex-M</description>
        <files>
          <file category="doc" name="CMSIS\Documentation\Driver\html\group__eth__phy__interface__gr.html" />
          <file category="header" name="CMSIS\Driver\Include\Driver_ETH_PHY.h" />
        </files>
      </api>
    <api Cclass="CMSIS Driver" Cgroup="USB Device" Capiversion="2.01" exclusive="0">
        <description>USB Device Driver API for Cortex-M</description>
        <files>
          <file category="doc" name="CMSIS\Documentation\Driver\html\group__usbd__interface__gr.html" />
          <file category="header" name="CMSIS\Driver\Include\Driver_USBD.h" />
        </files>
      </api>
    <api Cclass="CMSIS Driver" Cgroup="USB Host" Capiversion="2.01" exclusive="0">
        <description>USB Host Driver API for Cortex-M</description>
        <files>
          <file category="doc" name="CMSIS\Documentation\Driver\html\group__usbh__interface__gr.html" />
          <file category="header" name="CMSIS\Driver\Include\Driver_USBH.h" />
        </files>
      </api>
  </apis>

  <!-- conditions are dependency rules that can apply to a component or an individual file -->
  <conditions>
    <condition id="ARMCC">
      <require Tcompiler="ARMCC"/>
    </condition>

    <condition id="GCC">
      <require Tcompiler="GCC"/>
    </condition>

    <condition id="IAR">
      <require Tcompiler="IAR"/>
    </condition>

    <condition id="Cortex-M Device">
      <description>Cortex-M processor based device: one of CM0, CM0+, CM3, CM4, CM7, SC000, SC3000</description>
      <accept Dcore="Cortex-M0"/>
      <accept Dcore="Cortex-M0+"/>
      <accept Dcore="Cortex-M3"/>
      <accept Dcore="Cortex-M4"/>
      <accept Dcore="Cortex-M7"/>
      <accept Dcore="SC000"/>
      <accept Dcore="SC300"/>
    </condition>

    <condition id="Cortex-M CMSIS Device">
      <description>ARM Cortex-M device</description>
      <require condition="Cortex-M Device"/>
      <require Cclass="CMSIS" Cgroup="CORE"/>
    </condition>

    <condition id="CMSIS Core">
      <description>CMSIS CORE processor and device specific Startup files</description>
      <require condition="Cortex-M Device"/>
      <require Cclass="Device" Cgroup="Startup"/>
    </condition>

    <condition id="ARMCM0 CMSIS">
      <!-- conditions selecting Devices -->
      <description>Generic ARM Cortex-M0 device and CMSIS Core</description>
      <require Dvendor="ARM:82" Dname="ARMCM0"/>
      <require Cclass="CMSIS" Cgroup="CORE"/>
    </condition>

    <condition id="ARMCM0 CMSIS GCC">
      <!-- conditions selecting Devices -->
      <description>Generic ARM Cortex-M0 device and CMSIS Core requiring GCC</description>
      <require condition="ARMCM0 CMSIS"/>
      <require condition="GCC"/>
    </condition>

    <condition id="ARMCM0+ CMSIS">
      <description>Generic ARM Cortex-M0+ device and CMSIS Core</description>
      <require Dvendor="ARM:82" Dname="ARMCM0P"/>
      <require Cclass="CMSIS" Cgroup="CORE"/>
    </condition>

    <condition id="ARMCM0+ CMSIS GCC">
      <description>Generic ARM Cortex-M0+ device and CMSIS Core requiring GCC</description>
      <require condition="ARMCM0+ CMSIS"/>
      <require condition="GCC"/>
    </condition>

    <condition id="ARMCM3 CMSIS">
      <description>Generic ARM Cortex-M3 device and CMSIS Core</description>
      <require Dvendor="ARM:82" Dname="ARMCM3"/>
      <require Cclass="CMSIS" Cgroup="CORE"/>
    </condition>

    <condition id="ARMCM3 CMSIS GCC">
      <description>Generic ARM Cortex-M3 device and CMSIS Core requiring GCC</description>
      <require condition="ARMCM3 CMSIS"/>
      <require condition="GCC"/>
    </condition>

    <condition id="ARMCM4 CMSIS">
      <description>Generic ARM Cortex-M4 device and CMSIS Core</description>
      <require Dvendor="ARM:82" Dname="ARMCM4*"/>
      <require Cclass="CMSIS" Cgroup="CORE"/>
    </condition>

    <condition id="ARMCM4 CMSIS GCC">
      <description>Generic ARM Cortex-M4 device and CMSIS Core requiring GCC</description>
      <require condition="ARMCM4 CMSIS"/>
      <require condition="GCC"/>
    </condition>

    <condition id="ARMCM7 CMSIS">
      <description>Generic ARM Cortex-M7 device and CMSIS Core</description>
      <require Dvendor="ARM:82" Dname="ARMCM7*"/>
      <require Cclass="CMSIS" Cgroup="CORE"/>
    </condition>

    <condition id="ARMCM7 CMSIS GCC">
      <description>Generic ARM Cortex-M7 device and CMSIS Core requiring GCC</description>
      <require condition="ARMCM7 CMSIS"/>
      <require condition="GCC"/>
    </condition>

    <condition id="ARMSC000 CMSIS">
      <description>Generic ARM SC000 device and CMSIS Core</description>
      <require Dvendor="ARM:82" Dname="ARMSC000"/>
      <require Cclass="CMSIS" Cgroup="CORE"/>
    </condition>

    <condition id="ARMSC000 CMSIS GCC">
      <description>Generic ARM SC000 device and CMSIS Core requiring GCC</description>
      <require condition="ARMSC000 CMSIS"/>
      <require condition="GCC"/>
    </condition>

    <condition id="ARMSC300 CMSIS">
      <description>Generic ARM SC300 device and CMSIS Core</description>
      <require Dvendor="ARM:82" Dname="ARMSC300"/>
      <require Cclass="CMSIS" Cgroup="CORE"/>
    </condition>

    <condition id="ARMSC300 CMSIS GCC">
      <description>Generic ARM SC300 device and CMSIS Core requiring GCC</description>
      <require condition="ARMSC300 CMSIS"/>
      <require condition="GCC"/>
    </condition>

    <condition id="CMSIS DSP">
      <description>CMSIS DSP Library is for ARM Cortex-M Devices only and is prebuild for one of the compilers ARMCC, GCC or IAR</description>
      <require condition="Cortex-M CMSIS Device"/>
      <accept Tcompiler="GCC"/>
      <accept Tcompiler="ARMCC"/>
      <accept Tcompiler="IAR"/>
    </condition>

    <!-- ARMCC compiler -->
    <condition id="CM0_LE_ARMCC">
      <description>Cortex-M0 or Cortex-M0+ or SC000 processor based device in little endian mode for the ARM Compiler</description>
      <accept Dcore="Cortex-M0"/>
      <accept Dcore="Cortex-M0+"/>
      <accept Dcore="SC000"/>
      <require Dendian="Little-endian"/>
      <require Tcompiler="ARMCC"/>
    </condition>

    <condition id="CM0_BE_ARMCC">
      <description>Cortex-M0 or Cortex-M0+ or SC000 processor based device in big endian mode for the ARM Compiler</description>
      <accept Dcore="Cortex-M0"/>
      <accept Dcore="Cortex-M0+"/>
      <accept Dcore="SC000"/>
      <require Dendian="Big-endian"/>
      <require Tcompiler="ARMCC"/>
    </condition>

    <condition id="CM3_LE_ARMCC">
      <description>Cortex-M3 or SC300 processor based device in little endian mode for the ARM Compiler</description>
      <accept Dcore="Cortex-M3"/>
      <accept Dcore="SC300"/>
      <require Dendian="Little-endian"/>
      <require Tcompiler="ARMCC"/>
    </condition>

    <condition id="CM3_BE_ARMCC">
      <description>Cortex-M3 or SC300 processor based device in big endian mode for the ARM Compiler</description>
      <accept Dcore="Cortex-M3"/>
      <accept Dcore="SC300"/>
      <require Dendian="Big-endian"/>
      <require Tcompiler="ARMCC"/>
    </condition>

    <condition id="CM4_LE_ARMCC">
      <description>Cortex-M4 processor based device in little endian mode for the ARM Compiler</description>
      <require Dcore="Cortex-M4" Dfpu="NO_FPU" Dendian="Little-endian"/>
      <require Tcompiler="ARMCC"/>
    </condition>

    <condition id="CM4_BE_ARMCC">
      <description>Cortex-M4 processor based device in big endian mode for the ARM Compiler</description>
      <require Dcore="Cortex-M4" Dfpu="NO_FPU" Dendian="Big-endian"/>
      <require Tcompiler="ARMCC"/>
    </condition>

    <condition id="CM4F_LE_ARMCC">
      <description>Cortex-M4 processor based device using Floating Point Unit in little endian mode for the ARM Compiler</description>
      <require Dcore="Cortex-M4" Dfpu="FPU" Dendian="Little-endian"/>
      <require Tcompiler="ARMCC"/>
    </condition>

    <condition id="CM4F_BE_ARMCC">
      <description>Cortex-M4 processor based device using Floating Point Unit in big endian mode for the ARM Compiler</description>
      <require Dcore="Cortex-M4" Dfpu="FPU" Dendian="Big-endian"/>
      <require Tcompiler="ARMCC"/>
    </condition>
    
    <!-- XMC 4000 Series devices from Infineon require a special library -->
    <condition id="CM4_LE_ARMCC_STD">
      <description>Cortex-M4 processor based device in little endian mode for the ARM Compiler without Infineon devices</description>
      <require Dcore="Cortex-M4" Dfpu="NO_FPU" Dendian="Little-endian"/>
      <deny Dvendor="Infineon:7" Dname="XMC4*"/>
      <require Tcompiler="ARMCC"/>
    </condition>
    <condition id="CM4_LE_ARMCC_IFX">
      <description>Cortex-M4 processor based device in little endian mode for the ARM Compiler and Infineon devices</description>
      <require Dcore="Cortex-M4" Dfpu="NO_FPU" Dendian="Little-endian" Dvendor="Infineon:7" Dname="XMC4*"/>
      <require Tcompiler="ARMCC"/>
    </condition>
    <condition id="CM4F_LE_ARMCC_STD">
      <description>Cortex-M4 processor based device using Floating Point Unit in little endian mode for the ARM Compiler without Infineon devices</description>
      <require Dcore="Cortex-M4" Dfpu="FPU" Dendian="Little-endian"/>
      <deny Dvendor="Infineon:7" Dname="XMC4*"/>
      <require Tcompiler="ARMCC"/>
    </condition>
    <condition id="CM4F_LE_ARMCC_IFX">
      <description>Cortex-M4 processor based device using Floating Point Unit in little endian mode for the ARM Compiler and Infineon devices</description>
      <require Dcore="Cortex-M4" Dfpu="FPU" Dendian="Little-endian" Dvendor="Infineon:7" Dname="XMC4*"/>
      <require Tcompiler="ARMCC"/>
    </condition>

    <condition id="CM7_LE_ARMCC">
      <description>Cortex-M7 processor based device in little endian mode for the ARM Compiler</description>
      <require Dcore="Cortex-M7" Dfpu="NO_FPU" Dendian="Little-endian"/>
      <require Tcompiler="ARMCC"/>
    </condition>

    <condition id="CM7_BE_ARMCC">
      <description>Cortex-M7 processor based device in big endian mode for the ARM Compiler</description>
      <require Dcore="Cortex-M7" Dfpu="NO_FPU" Dendian="Big-endian"/>
      <require Tcompiler="ARMCC"/>
    </condition>

    <condition id="CM7F_LE_ARMCC">
      <description>Cortex-M7 processor based device using Floating Point Unit in little endian mode for the ARM Compiler</description>
      <accept Dcore="Cortex-M7" Dfpu="SP_FPU" Dendian="Little-endian"/>
      <accept Dcore="Cortex-M7" Dfpu="DP_FPU" Dendian="Little-endian"/>
      <require Tcompiler="ARMCC"/>
    </condition>

    <condition id="CM7F_BE_ARMCC">
      <description>Cortex-M7 processor based device using Floating Point Unit in big endian mode for the ARM Compiler</description>
      <accept Dcore="Cortex-M7" Dfpu="SP_FPU" Dendian="Big-endian"/>
      <accept Dcore="Cortex-M7" Dfpu="DP_FPU" Dendian="Big-endian"/>
      <require Tcompiler="ARMCC"/>
    </condition>

    <condition id="CM7FSP_LE_ARMCC">
      <description>Cortex-M7 processor based device using Floating Point Unit in little endian mode for the ARM Compiler</description>
      <accept Dcore="Cortex-M7" Dfpu="SP_FPU" Dendian="Little-endian"/>
      <require Tcompiler="ARMCC"/>
    </condition>

    <condition id="CM7FSP_BE_ARMCC">
      <description>Cortex-M7 processor based device using Floating Point Unit in big endian mode for the ARM Compiler</description>
      <accept Dcore="Cortex-M7" Dfpu="SP_FPU" Dendian="Big-endian"/>
      <require Tcompiler="ARMCC"/>
    </condition>

    <condition id="CM7FDP_LE_ARMCC">
      <description>Cortex-M7 processor based device using Floating Point Unit in little endian mode for the ARM Compiler</description>
      <accept Dcore="Cortex-M7" Dfpu="DP_FPU" Dendian="Little-endian"/>
      <require Tcompiler="ARMCC"/>
    </condition>

    <condition id="CM7FDP_BE_ARMCC">
      <description>Cortex-M7 processor based device using Floating Point Unit in big endian mode for the ARM Compiler</description>
      <accept Dcore="Cortex-M7" Dfpu="DP_FPU" Dendian="Big-endian"/>
      <require Tcompiler="ARMCC"/>
    </condition>

    <!-- GCC compiler -->
    <condition id="CM0_LE_GCC">
      <description>Cortex-M0 or Cortex-M0+ or SC000 processor based device in little endian mode for the GCC Compiler</description>
      <accept Dcore="Cortex-M0"/>
      <accept Dcore="Cortex-M0+"/>
      <accept Dcore="SC000"/>
      <require Dendian="Little-endian"/>
      <require Tcompiler="GCC"/>
    </condition>

    <condition id="CM0_BE_GCC">
      <description>Cortex-M0 or Cortex-M0+ or SC000 processor based device in big endian mode for the GCC Compiler</description>
      <accept Dcore="Cortex-M0"/>
      <accept Dcore="Cortex-M0+"/>
      <accept Dcore="SC000"/>
      <require Dendian="Big-endian"/>
      <require Tcompiler="GCC"/>
    </condition>

    <condition id="CM3_LE_GCC">
      <description>Cortex-M3 or SC300 processor based device in little endian mode for the GCC Compiler</description>
      <accept Dcore="Cortex-M3"/>
      <accept Dcore="SC300"/>
      <require Dendian="Little-endian"/>
      <require Tcompiler="GCC"/>
    </condition>

    <condition id="CM3_BE_GCC">
      <description>Cortex-M3 or SC300 processor based device in big endian mode for the GCC Compiler</description>
      <accept Dcore="Cortex-M3"/>
      <accept Dcore="SC300"/>
      <require Dendian="Big-endian"/>
      <require Tcompiler="GCC"/>
    </condition>

    <condition id="CM4_LE_GCC">
      <description>Cortex-M4 processor based device in little endian mode for the GCC Compiler</description>
      <require Dcore="Cortex-M4" Dfpu="NO_FPU" Dendian="Little-endian"/>
      <require Tcompiler="GCC"/>
    </condition>

    <condition id="CM4_BE_GCC">
      <description>Cortex-M4 processor based device in big endian mode for the GCC Compiler</description>
      <require Dcore="Cortex-M4" Dfpu="NO_FPU" Dendian="Big-endian"/>
      <require Tcompiler="GCC"/>
    </condition>

    <condition id="CM4F_LE_GCC">
      <description>Cortex-M4 processor based device using Floating Point Unit in little endian mode for the GCC Compiler</description>
      <require Dcore="Cortex-M4" Dfpu="FPU" Dendian="Little-endian"/>
      <require Tcompiler="GCC"/>
    </condition>

    <condition id="CM4F_BE_GCC">
      <description>Cortex-M4 processor based device using Floating Point Unit in big endian mode for the GCC Compiler</description>
      <require Dcore="Cortex-M4" Dfpu="FPU" Dendian="Big-endian"/>
      <require Tcompiler="GCC"/>
    </condition>

    <!-- XMC 4000 Series devices from Infineon require a special library -->
    <condition id="CM4_LE_GCC_STD">
      <description>Cortex-M4 processor based device in little endian mode for the GCC Compiler without Infineon devices</description>
      <require Dcore="Cortex-M4" Dfpu="NO_FPU" Dendian="Little-endian"/>
      <deny Dvendor="Infineon:7" Dname="XMC4*"/>
      <require Tcompiler="GCC"/>
    </condition>
    <condition id="CM4_LE_GCC_IFX">
      <description>Cortex-M4 processor based device in little endian mode for the GCC Compiler and Infineon devices</description>
      <require Dcore="Cortex-M4" Dfpu="NO_FPU" Dendian="Little-endian" Dvendor="Infineon:7" Dname="XMC4*"/>
      <require Tcompiler="GCC"/>
    </condition>
    <condition id="CM4F_LE_GCC_STD">
      <description>Cortex-M4 processor based device using Floating Point Unit in little endian mode for the GCC Compiler without Infineon devices</description>
      <require Dcore="Cortex-M4" Dfpu="FPU" Dendian="Little-endian"/>
      <deny Dvendor="Infineon:7" Dname="XMC4*"/>
      <require Tcompiler="GCC"/>
    </condition>
    <condition id="CM4F_LE_GCC_IFX">
      <description>Cortex-M4 processor based device using Floating Point Unit in little endian mode for the GCC Compiler and Infineon devices</description>
      <require Dcore="Cortex-M4" Dfpu="FPU" Dendian="Little-endian" Dvendor="Infineon:7" Dname="XMC4*"/>
      <require Tcompiler="GCC"/>
    </condition>

    <condition id="CM7_LE_GCC">
      <description>Cortex-M7 processor based device in little endian mode for the GCC Compiler</description>
      <require Dcore="Cortex-M7" Dfpu="NO_FPU" Dendian="Little-endian"/>
      <require Tcompiler="GCC"/>
    </condition>

    <condition id="CM7_BE_GCC">
      <description>Cortex-M7 processor based device in big endian mode for the GCC Compiler</description>
      <require Dcore="Cortex-M7" Dfpu="NO_FPU" Dendian="Big-endian"/>
      <require Tcompiler="GCC"/>
    </condition>

    <condition id="CM7F_LE_GCC">
      <description>Cortex-M7 processor based device using Floating Point Unit in little endian mode for the GCC Compiler</description>
      <accept Dcore="Cortex-M7" Dfpu="SP_FPU" Dendian="Little-endian"/>
      <accept Dcore="Cortex-M7" Dfpu="DP_FPU" Dendian="Little-endian"/>
      <require Tcompiler="GCC"/>
    </condition>

    <condition id="CM7F_BE_GCC">
      <description>Cortex-M7 processor based device using Floating Point Unit in big endian mode for the GCC Compiler</description>
      <accept Dcore="Cortex-M7" Dfpu="SP_FPU" Dendian="Big-endian"/>
      <accept Dcore="Cortex-M7" Dfpu="DP_FPU" Dendian="Big-endian"/>
      <require Tcompiler="GCC"/>
    </condition>

    <condition id="CM7FSP_LE_GCC">
      <description>Cortex-M7 processor based device using Floating Point Unit in little endian mode for the GCC Compiler</description>
      <accept Dcore="Cortex-M7" Dfpu="SP_FPU" Dendian="Little-endian"/>
      <require Tcompiler="GCC"/>
    </condition>

    <condition id="CM7FSP_BE_GCC">
      <description>Cortex-M7 processor based device using Floating Point Unit in big endian mode for the GCC Compiler</description>
      <accept Dcore="Cortex-M7" Dfpu="SP_FPU" Dendian="Big-endian"/>
      <require Tcompiler="GCC"/>
    </condition>

    <condition id="CM7FDP_LE_GCC">
      <description>Cortex-M7 processor based device using Floating Point Unit in little endian mode for the GCC Compiler</description>
      <accept Dcore="Cortex-M7" Dfpu="DP_FPU" Dendian="Little-endian"/>
      <require Tcompiler="GCC"/>
    </condition>

    <condition id="CM7FDP_BE_GCC">
      <description>Cortex-M7 processor based device using Floating Point Unit in big endian mode for the GCC Compiler</description>
      <accept Dcore="Cortex-M7" Dfpu="DP_FPU" Dendian="Big-endian"/>
      <require Tcompiler="GCC"/>
    </condition>

    <!-- IAR compiler -->
    <condition id="CM0_LE_IAR">
      <description>Cortex-M0 or Cortex-M0+ or SC000 processor based device in little endian mode for the IAR Compiler</description>
      <accept Dcore="Cortex-M0"/>
      <accept Dcore="Cortex-M0+"/>
      <accept Dcore="SC000"/>
      <require Dendian="Little-endian"/>
      <require Tcompiler="IAR"/>
    </condition>

    <condition id="CM0_BE_IAR">
      <description>Cortex-M0 or Cortex-M0+ or SC000 processor based device in big endian mode for the IAR Compiler</description>
      <accept Dcore="Cortex-M0"/>
      <accept Dcore="Cortex-M0+"/>
      <accept Dcore="SC000"/>
      <require Dendian="Big-endian"/>
      <require Tcompiler="IAR"/>
    </condition>

    <condition id="CM3_LE_IAR">
      <description>Cortex-M3 or SC300 processor based device in little endian mode for the IAR Compiler</description>
      <accept Dcore="Cortex-M3"/>
      <accept Dcore="SC300"/>
      <require Dendian="Little-endian"/>
      <require Tcompiler="IAR"/>
    </condition>

    <condition id="CM3_BE_IAR">
      <description>Cortex-M3 or SC300 processor based device in big endian mode for the IAR Compiler</description>
      <accept Dcore="Cortex-M3"/>
      <accept Dcore="SC300"/>
      <require Dendian="Big-endian"/>
      <require Tcompiler="IAR"/>
    </condition>

    <condition id="CM4_LE_IAR">
      <description>Cortex-M4 processor based device in little endian mode for the IAR Compiler</description>
      <require Dcore="Cortex-M4" Dfpu="NO_FPU" Dendian="Little-endian"/>
      <require Tcompiler="IAR"/>
    </condition>

    <condition id="CM4_BE_IAR">
      <description>Cortex-M4 processor based device in big endian mode for the IAR Compiler</description>
      <require Dcore="Cortex-M4" Dfpu="NO_FPU" Dendian="Big-endian"/>
      <require Tcompiler="IAR"/>
    </condition>

    <condition id="CM4F_LE_IAR">
      <description>Cortex-M4 processor based device using Floating Point Unit in little endian mode for the IAR Compiler</description>
      <require Dcore="Cortex-M4" Dfpu="FPU" Dendian="Little-endian"/>
      <require Tcompiler="IAR"/>
    </condition>

    <condition id="CM4F_BE_IAR">
      <description>Cortex-M4 processor based device using Floating Point Unit in big endian mode for the IAR Compiler</description>
      <require Dcore="Cortex-M4" Dfpu="FPU" Dendian="Big-endian"/>
      <require Tcompiler="IAR"/>
    </condition>

    <condition id="CM7_LE_IAR">
      <description>Cortex-M7 processor based device in little endian mode for the IAR Compiler</description>
      <require Dcore="Cortex-M7" Dfpu="NO_FPU" Dendian="Little-endian"/>
      <require Tcompiler="IAR"/>
    </condition>

    <condition id="CM7_BE_IAR">
      <description>Cortex-M7 processor based device in big endian mode for the IAR Compiler</description>
      <require Dcore="Cortex-M7" Dfpu="NO_FPU" Dendian="Big-endian"/>
      <require Tcompiler="IAR"/>
    </condition>

    <condition id="CM7F_LE_IAR">
      <description>Cortex-M7 processor based device using Floating Point Unit in little endian mode for the IAR Compiler</description>
      <accept Dcore="Cortex-M7" Dfpu="SP_FPU" Dendian="Little-endian"/>
      <accept Dcore="Cortex-M7" Dfpu="DP_FPU" Dendian="Little-endian"/>
      <require Tcompiler="IAR"/>
    </condition>

    <condition id="CM7F_BE_IAR">
      <description>Cortex-M7 processor based device using Floating Point Unit in big endian mode for the IAR Compiler</description>
      <accept Dcore="Cortex-M7" Dfpu="SP_FPU" Dendian="Big-endian"/>
      <accept Dcore="Cortex-M7" Dfpu="DP_FPU" Dendian="Big-endian"/>
      <require Tcompiler="IAR"/>
    </condition>

    <condition id="CM7FSP_LE_IAR">
      <description>Cortex-M7 processor based device using Floating Point Unit in little endian mode for the IAR Compiler</description>
      <accept Dcore="Cortex-M7" Dfpu="SP_FPU" Dendian="Little-endian"/>
      <require Tcompiler="IAR"/>
    </condition>

    <condition id="CM7FSP_BE_IAR">
      <description>Cortex-M7 processor based device using Floating Point Unit in big endian mode for the IAR Compiler</description>
      <accept Dcore="Cortex-M7" Dfpu="SP_FPU" Dendian="Big-endian"/>
      <require Tcompiler="IAR"/>
    </condition>

    <condition id="CM7FDP_LE_IAR">
      <description>Cortex-M7 processor based device using Floating Point Unit in little endian mode for the IAR Compiler</description>
      <accept Dcore="Cortex-M7" Dfpu="DP_FPU" Dendian="Little-endian"/>
      <require Tcompiler="IAR"/>
    </condition>

    <condition id="CM7FDP_BE_IAR">
      <description>Cortex-M7 processor based device using Floating Point Unit in big endian mode for the IAR Compiler</description>
      <accept Dcore="Cortex-M7" Dfpu="DP_FPU" Dendian="Big-endian"/>
      <require Tcompiler="IAR"/>
    </condition>
  </conditions>
  
  <components>
    <!-- CMSIS-Core component -->
    <component Cclass="CMSIS" Cgroup="CORE" Cversion="3.40.0" condition="CMSIS Core">
      <description>CMSIS-CORE for Cortex-M, SC000, and SC300</description>
      <files>
        <!-- templates -->
        <file category="source" attr="template" name="CMSIS\UserCodeTemplates\ARM\ITM_Retarget.c" select="CMSIS-CORE 'ITM Printf Debug'" condition="ARMCC"/>
        <!-- CPU independent -->
        <file category="doc"     name="CMSIS\Documentation\Core\html\index.html"/>
        <file category="include" name="CMSIS\Include\"/>
      </files>
    </component>

    <!-- CMSIS-Startup components -->
    <!-- Cortex-M0 -->
    <component Cclass="Device" Cgroup="Startup" Cversion="1.0.1" condition="ARMCM0 CMSIS">
      <description>System and Startup for Generic ARM Cortex-M0 device</description>
      <files>
        <!-- include folder / device header file -->
        <file category="header"  name="Device\ARM\ARMCM0\Include\ARMCM0.h"/>
        <!-- startup / system file -->
        <file category="sourceAsm"    name="Device\ARM\ARMCM0\Source\ARM\startup_ARMCM0.s" version="1.0.0" attr="config" condition="ARMCC"/>
        <file category="sourceAsm"    name="Device\ARM\ARMCM0\Source\GCC\startup_ARMCM0.S" version="1.0.0" attr="config" condition="GCC"/>
        <file category="linkerScript" name="Device\ARM\ARMCM0\Source\GCC\gcc_arm.ld"       version="1.0.0" attr="config" condition="GCC"/>
        <file category="sourceAsm"    name="Device\ARM\ARMCM0\Source\IAR\startup_ARMCM0.s" version="1.0.0" attr="config" condition="IAR"/>
        <file category="sourceC"      name="Device\ARM\ARMCM0\Source\system_ARMCM0.c"      version="1.0.0" attr="config"/>
      </files>
    </component>
    <component Cclass="Device" Cgroup="Startup" Cvariant="C Startup"   Cversion="1.0.1" condition="ARMCM0 CMSIS GCC">
      <description>System and Startup for Generic ARM Cortex-M0 device</description>
      <files>
        <!-- include folder / device header file -->
        <file category="header"  name="Device\ARM\ARMCM0\Include\ARMCM0.h"/>
        <!-- startup / system file -->
        <file category="sourceC"      name="Device\ARM\ARMCM0\Source\GCC\startup_ARMCM0.c" version="1.0.0" attr="config" condition="GCC"/>
        <file category="linkerScript" name="Device\ARM\ARMCM0\Source\GCC\gcc_arm.ld"       version="1.0.0" attr="config" condition="GCC"/>
        <file category="sourceC"      name="Device\ARM\ARMCM0\Source\system_ARMCM0.c"      version="1.0.0" attr="config"/>
      </files>
    </component>

    <!-- Cortex-M0+ -->
    <component Cclass="Device" Cgroup="Startup" Cversion="1.0.1" condition="ARMCM0+ CMSIS">
      <description>System and Startup for Generic ARM Cortex-M0+ device</description>
      <files>
        <!-- include folder / device header file -->
        <file category="header"  name="Device\ARM\ARMCM0plus\Include\ARMCM0plus.h"/>
        <!-- startup / system file -->
        <file category="sourceAsm"    name="Device\ARM\ARMCM0plus\Source\ARM\startup_ARMCM0plus.s" version="1.0.0" attr="config" condition="ARMCC"/>
        <file category="sourceAsm"    name="Device\ARM\ARMCM0plus\Source\GCC\startup_ARMCM0plus.S" version="1.0.0" attr="config" condition="GCC"/>
        <file category="linkerScript" name="Device\ARM\ARMCM0plus\Source\GCC\gcc_arm.ld"           version="1.0.0" attr="config" condition="GCC"/>
        <file category="sourceAsm"    name="Device\ARM\ARMCM0plus\Source\IAR\startup_ARMCM0plus.s" version="1.0.0" attr="config" condition="IAR"/>
        <file category="sourceC"      name="Device\ARM\ARMCM0plus\Source\system_ARMCM0plus.c"      version="1.0.0" attr="config"/>
      </files>
    </component>
    <component Cclass="Device" Cgroup="Startup" Cvariant="C Startup"   Cversion="1.0.1" condition="ARMCM0+ CMSIS GCC">
      <description>System and Startup for Generic ARM Cortex-M0+ device</description>
      <files>
        <!-- include folder / device header file -->
        <file category="header"  name="Device\ARM\ARMCM0plus\Include\ARMCM0plus.h"/>
        <!-- startup / system file -->
        <file category="sourceC"      name="Device\ARM\ARMCM0plus\Source\GCC\startup_ARMCM0plus.c" version="1.0.0" attr="config" condition="GCC"/>
        <file category="linkerScript" name="Device\ARM\ARMCM0plus\Source\GCC\gcc_arm.ld"           version="1.0.0" attr="config" condition="GCC"/>
        <file category="sourceC"      name="Device\ARM\ARMCM0plus\Source\system_ARMCM0plus.c"      version="1.0.0" attr="config"/>
      </files>
    </component>

    <!-- Cortex-M3 -->
    <component Cclass="Device" Cgroup="Startup" Cversion="1.0.1" condition="ARMCM3 CMSIS">
      <description>System and Startup for Generic ARM Cortex-M3 device</description>
      <files>
        <!-- include folder / device header file -->
        <file category="header"  name="Device\ARM\ARMCM3\Include\ARMCM3.h"/>
        <!-- startup / system file -->
        <file category="sourceAsm"    name="Device\ARM\ARMCM3\Source\ARM\startup_ARMCM3.s" version="1.0.0" attr="config" condition="ARMCC"/>
        <file category="sourceAsm"    name="Device\ARM\ARMCM3\Source\GCC\startup_ARMCM3.S" version="1.0.0" attr="config" condition="GCC"/>
        <file category="linkerScript" name="Device\ARM\ARMCM3\Source\GCC\gcc_arm.ld"       version="1.0.0" attr="config" condition="GCC"/>
        <file category="sourceAsm"    name="Device\ARM\ARMCM3\Source\IAR\startup_ARMCM3.s" version="1.0.0" attr="config" condition="IAR"/>
        <file category="sourceC"      name="Device\ARM\ARMCM3\Source\system_ARMCM3.c"      version="1.0.0" attr="config"/>
      </files>
    </component>
    <component Cclass="Device" Cgroup="Startup" Cvariant="C Startup"   Cversion="1.0.1" condition="ARMCM3 CMSIS GCC">
      <description>System and Startup for Generic ARM Cortex-M3 device</description>
      <files>
        <!-- include folder / device header file -->
        <file category="header"  name="Device\ARM\ARMCM3\Include\ARMCM3.h"/>
        <!-- startup / system file -->
        <file category="sourceC"      name="Device\ARM\ARMCM3\Source\GCC\startup_ARMCM3.c" version="1.0.0" attr="config" condition="GCC"/>
        <file category="linkerScript" name="Device\ARM\ARMCM3\Source\GCC\gcc_arm.ld"       version="1.0.0" attr="config" condition="GCC"/>
        <file category="sourceC"      name="Device\ARM\ARMCM3\Source\system_ARMCM3.c"      version="1.0.0" attr="config"/>
      </files>
    </component>

    <!-- Cortex-M4 -->
    <component Cclass="Device" Cgroup="Startup" Cversion="1.0.1" condition="ARMCM4 CMSIS">
      <description>System and Startup for Generic ARM Cortex-M4 device</description>
      <files>
        <!-- include folder / device header file -->
        <file category="include" name="Device\ARM\ARMCM4\Include\"/>
        <!-- startup / system file -->
        <file category="sourceAsm"    name="Device\ARM\ARMCM4\Source\ARM\startup_ARMCM4.s" version="1.0.0" attr="config" condition="ARMCC"/>
        <file category="sourceAsm"    name="Device\ARM\ARMCM4\Source\GCC\startup_ARMCM4.S" version="1.0.0" attr="config" condition="GCC"/>
        <file category="linkerScript" name="Device\ARM\ARMCM4\Source\GCC\gcc_arm.ld"       version="1.0.0" attr="config" condition="GCC"/>
        <file category="sourceAsm"    name="Device\ARM\ARMCM4\Source\IAR\startup_ARMCM4.s" version="1.0.0" attr="config" condition="IAR"/>
        <file category="sourceC"      name="Device\ARM\ARMCM4\Source\system_ARMCM4.c"      version="1.0.0" attr="config"/>
      </files>
    </component>
    <component Cclass="Device" Cgroup="Startup" Cvariant="C Startup"   Cversion="1.0.1" condition="ARMCM4 CMSIS GCC">
      <description>System and Startup for Generic ARM Cortex-M4 device</description>
      <files>
        <!-- include folder / device header file -->
        <file category="include" name="Device\ARM\ARMCM4\Include\"/>
        <!-- startup / system file -->
        <file category="sourceC"      name="Device\ARM\ARMCM4\Source\GCC\startup_ARMCM4.c" version="1.0.0" attr="config" condition="GCC"/>
        <file category="linkerScript" name="Device\ARM\ARMCM4\Source\GCC\gcc_arm.ld"       version="1.0.0" attr="config" condition="GCC"/>
        <file category="sourceC"      name="Device\ARM\ARMCM4\Source\system_ARMCM4.c"      version="1.0.0" attr="config"/>
      </files>
    </component>

    <!-- Cortex-M7 -->
    <component Cclass="Device" Cgroup="Startup" Cversion="1.0.1" condition="ARMCM7 CMSIS">
      <description>System and Startup for Generic ARM Cortex-M7 device</description>
      <files>
        <!-- include folder / device header file -->
        <file category="include"  name="Device\ARM\ARMCM7\Include\"/>
        <!-- startup / system file -->
        <file category="sourceAsm"    name="Device\ARM\ARMCM7\Source\ARM\startup_ARMCM7.s" version="1.0.0" attr="config" condition="ARMCC"/>
        <file category="sourceAsm"    name="Device\ARM\ARMCM7\Source\GCC\startup_ARMCM7.S" version="1.0.0" attr="config" condition="GCC"/>
        <file category="linkerScript" name="Device\ARM\ARMCM7\Source\GCC\gcc_arm.ld"       version="1.0.0" attr="config" condition="GCC"/>
        <file category="sourceAsm"    name="Device\ARM\ARMCM7\Source\IAR\startup_ARMCM7.s" version="1.0.0" attr="config" condition="IAR"/>
        <file category="sourceC"      name="Device\ARM\ARMCM7\Source\system_ARMCM7.c"      version="1.0.0" attr="config"/>
      </files>
    </component>
    <component Cclass="Device" Cgroup="Startup" Cvariant="C Startup"   Cversion="1.0.1" condition="ARMCM7 CMSIS GCC">
      <description>System and Startup for Generic ARM Cortex-M4 device</description>
      <files>
        <!-- include folder / device header file -->
        <file category="include"  name="Device\ARM\ARMCM7\Include\"/>
        <!-- startup / system file -->
        <file category="sourceC"      name="Device\ARM\ARMCM7\Source\GCC\startup_ARMCM7.c" version="1.0.0" attr="config" condition="GCC"/>
        <file category="linkerScript" name="Device\ARM\ARMCM7\Source\GCC\gcc_arm.ld"       version="1.0.0" attr="config" condition="GCC"/>
        <file category="sourceC"      name="Device\ARM\ARMCM7\Source\system_ARMCM7.c"      version="1.0.0" attr="config"/>
      </files>
    </component>

    <!-- Cortex-SC000 -->
    <component Cclass="Device" Cgroup="Startup" Cversion="1.0.1" condition="ARMSC000 CMSIS">
      <description>System and Startup for Generic ARM SC000 device</description>
      <files>
        <!-- include folder / device header file -->
        <file category="header"  name="Device\ARM\ARMSC000\Include\ARMSC000.h"/>
        <!-- startup / system file -->
        <file category="sourceAsm"    name="Device\ARM\ARMSC000\Source\ARM\startup_ARMSC000.s" version="1.0.0" attr="config" condition="ARMCC"/>
        <file category="sourceAsm"    name="Device\ARM\ARMSC000\Source\GCC\startup_ARMSC000.S" version="1.0.0" attr="config" condition="GCC"/>
        <file category="linkerScript" name="Device\ARM\ARMSC000\Source\GCC\gcc_arm.ld"         version="1.0.0" attr="config" condition="GCC"/>
        <file category="sourceAsm"    name="Device\ARM\ARMSC000\Source\IAR\startup_ARMSC000.s" version="1.0.0" attr="config" condition="IAR"/>
        <file category="sourceC"      name="Device\ARM\ARMSC000\Source\system_ARMSC000.c"      version="1.0.0" attr="config"/>
      </files>
    </component>
    <component Cclass="Device" Cgroup="Startup" Cvariant="C Startup"   Cversion="1.0.1" condition="ARMSC000 CMSIS GCC">
      <description>System and Startup for Generic ARM SC000 device</description>
      <files>
        <!-- include folder / device header file -->
        <file category="header"  name="Device\ARM\ARMSC000\Include\ARMSC000.h"/>
        <!-- startup / system file -->
        <file category="sourceC"      name="Device\ARM\ARMSC000\Source\GCC\startup_ARMSC000.c" version="1.0.0" attr="config" condition="GCC"/>
        <file category="linkerScript" name="Device\ARM\ARMSC000\Source\GCC\gcc_arm.ld"         version="1.0.0" attr="config" condition="GCC"/>
        <file category="sourceC"      name="Device\ARM\ARMSC000\Source\system_ARMSC000.c"      version="1.0.0" attr="config"/>
      </files>
    </component>

    <!-- Cortex-SC300 -->
    <component Cclass="Device" Cgroup="Startup" Cversion="1.0.1" condition="ARMSC300 CMSIS">
      <description>System and Startup for Generic ARM SC300 device</description>
      <files>
        <!-- include folder / device header file -->
        <file category="header"  name="Device\ARM\ARMSC300\Include\ARMSC300.h"/>
        <!-- startup / system file -->
        <file category="sourceAsm"    name="Device\ARM\ARMSC300\Source\ARM\startup_ARMSC300.s" version="1.0.0" attr="config" condition="ARMCC"/>
        <file category="sourceAsm"    name="Device\ARM\ARMSC300\Source\GCC\startup_ARMSC300.S" version="1.0.0" attr="config" condition="GCC"/>
        <file category="linkerScript" name="Device\ARM\ARMSC300\Source\GCC\gcc_arm.ld"         version="1.0.0" attr="config" condition="GCC"/>
        <file category="sourceAsm"    name="Device\ARM\ARMSC300\Source\IAR\startup_ARMSC300.s" version="1.0.0" attr="config" condition="IAR"/>
        <file category="sourceC"      name="Device\ARM\ARMSC300\Source\system_ARMSC300.c"      version="1.0.0" attr="config"/>
      </files>
    </component>
    <component Cclass="Device" Cgroup="Startup" Cvariant="C Startup"   Cversion="1.0.1" condition="ARMSC300 CMSIS GCC">
      <description>System and Startup for Generic ARM SC300 device</description>
      <files>
        <!-- include folder / device header file -->
        <file category="header"  name="Device\ARM\ARMSC300\Include\ARMSC300.h"/>
        <!-- startup / system file -->
        <file category="sourceC"      name="Device\ARM\ARMSC300\Source\GCC\startup_ARMSC300.c" version="1.0.0" attr="config" condition="GCC"/>
        <file category="linkerScript" name="Device\ARM\ARMSC300\Source\GCC\gcc_arm.ld"         version="1.0.0" attr="config" condition="GCC"/>
        <file category="sourceC"      name="Device\ARM\ARMSC300\Source\system_ARMSC300.c"      version="1.0.0" attr="config"/>
      </files>
    </component>

    <!-- CMSIS-DSP component -->
    <component Cclass="CMSIS" Cgroup="DSP" Cversion="1.4.2" condition="CMSIS DSP">
      <description>CMSIS-DSP Library for Cortex-M, SC000, and SC300</description>
      <files>
        <!-- CPU independent -->
        <file category="doc" name="CMSIS\Documentation\DSP\html\index.html"/>
        <!-- <file category="header" name="CMSIS\Include\arm_common_tables.h"/> -->
        <file category="header" name="CMSIS\Include\arm_math.h"/>
        <!-- CPU and Compiler dependent -->
        <!-- ARMCC -->
        <file category="library" condition="CM0_LE_ARMCC"     name="CMSIS\Lib\ARM\arm_cortexM0l_math.lib"      src="CMSIS\DSP_Lib\Source\ARM"/>
        <file category="library" condition="CM0_BE_ARMCC"     name="CMSIS\Lib\ARM\arm_cortexM0b_math.lib"      src="CMSIS\DSP_Lib\Source\ARM"/>
        <file category="library" condition="CM3_LE_ARMCC"     name="CMSIS\Lib\ARM\arm_cortexM3l_math.lib"      src="CMSIS\DSP_Lib\Source\ARM"/>
        <file category="library" condition="CM3_BE_ARMCC"     name="CMSIS\Lib\ARM\arm_cortexM3b_math.lib"      src="CMSIS\DSP_Lib\Source\ARM"/>
        <file category="library" condition="CM4_LE_ARMCC"     name="CMSIS\Lib\ARM\arm_cortexM4l_math.lib"      src="CMSIS\DSP_Lib\Source\ARM"/>
        <file category="library" condition="CM4_BE_ARMCC"     name="CMSIS\Lib\ARM\arm_cortexM4b_math.lib"      src="CMSIS\DSP_Lib\Source\ARM"/>
        <file category="library" condition="CM4F_LE_ARMCC"    name="CMSIS\Lib\ARM\arm_cortexM4lf_math.lib"     src="CMSIS\DSP_Lib\Source\ARM"/>
        <file category="library" condition="CM4F_BE_ARMCC"    name="CMSIS\Lib\ARM\arm_cortexM4bf_math.lib"     src="CMSIS\DSP_Lib\Source\ARM"/>
        <file category="library" condition="CM7_LE_ARMCC"     name="CMSIS\Lib\ARM\arm_cortexM7l_math.lib"      src="CMSIS\DSP_Lib\Source\ARM"/>
        <file category="library" condition="CM7_BE_ARMCC"     name="CMSIS\Lib\ARM\arm_cortexM7b_math.lib"      src="CMSIS\DSP_Lib\Source\ARM"/>
        <file category="library" condition="CM7FSP_LE_ARMCC"  name="CMSIS\Lib\ARM\arm_cortexM7lfsp_math.lib"   src="CMSIS\DSP_Lib\Source\ARM"/>
        <file category="library" condition="CM7FSP_BE_ARMCC"  name="CMSIS\Lib\ARM\arm_cortexM7bfsp_math.lib"   src="CMSIS\DSP_Lib\Source\ARM"/>
        <file category="library" condition="CM7FDP_LE_ARMCC"  name="CMSIS\Lib\ARM\arm_cortexM7lfdp_math.lib"   src="CMSIS\DSP_Lib\Source\ARM"/>
        <file category="library" condition="CM7FDP_BE_ARMCC"  name="CMSIS\Lib\ARM\arm_cortexM7bfdp_math.lib"   src="CMSIS\DSP_Lib\Source\ARM"/>
        <!-- GCC -->
        <file category="library" condition="CM0_LE_GCC"       name="CMSIS\Lib\GCC\libarm_cortexM0l_math.a"     src="CMSIS\DSP_Lib\Source\GCC"/>
        <file category="library" condition="CM3_LE_GCC"       name="CMSIS\Lib\GCC\libarm_cortexM3l_math.a"     src="CMSIS\DSP_Lib\Source\GCC"/>
        <file category="library" condition="CM4_LE_GCC"       name="CMSIS\Lib\GCC\libarm_cortexM4l_math.a"     src="CMSIS\DSP_Lib\Source\GCC"/>
        <file category="library" condition="CM4F_LE_GCC"      name="CMSIS\Lib\GCC\libarm_cortexM4lf_math.a"    src="CMSIS\DSP_Lib\Source\GCC"/>
        <!--file category="library" condition="CM7_LE_GCC"       name="CMSIS\Lib\GCC\libarm_cortexM7l_math.a"     src="CMSIS\DSP_Lib\Source\GCC"/-->
        <!--file category="library" condition="CM7FSP_LE_GCC"    name="CMSIS\Lib\GCC\libarm_cortexM7lfsp_math.a"  src="CMSIS\DSP_Lib\Source\GCC"/-->
        <!--file category="library" condition="CM7FDP_LE_GCC"    name="CMSIS\Lib\GCC\libarm_cortexM7lfdp_math.a"  src="CMSIS\DSP_Lib\Source\GCC"/-->
      </files>
    </component>

    <!-- CMSIS-RTOS Keil RTX component -->
    <component Cclass="CMSIS" Cgroup="RTOS" Csub="Keil RTX" Cversion="4.75.0" condition="CMSIS Core">
      <description>CMSIS-RTOS RTX implementation for Cortex-M, SC000, and SC300</description>
      <RTE_Components_h>
        <!-- the following content goes into file 'RTE_Components.h' -->
        #define RTE_CMSIS_RTOS                  /* CMSIS-RTOS */
        #define RTE_CMSIS_RTOS_RTX              /* CMSIS-RTOS Keil RTX */
      </RTE_Components_h>
      <files>
        <!-- CPU independent -->
        <file category="doc" name="CMSIS_RTX\Doc\index.html"/>
        <file category="header" name="CMSIS_RTX\INC\cmsis_os.h"/>
        <file category="source" attr="config"   name="CMSIS_RTX\Templates\RTX_Conf_CM.c" version="4.70"/>
        
        <!-- RTX templates -->
        <file category="header" attr="template" name="CMSIS_RTX\UserCodeTemplates\osObjects.h" select="CMSIS-RTOS 'main' function"/>
        <file category="source" attr="template" name="CMSIS_RTX\UserCodeTemplates\main.c"      select="CMSIS-RTOS 'main' function"/>
        <file category="source" attr="template" name="CMSIS_RTX\UserCodeTemplates\MailQueue.c" select="CMSIS-RTOS Mail Queue"/>
        <file category="source" attr="template" name="CMSIS_RTX\UserCodeTemplates\MemPool.c"   select="CMSIS-RTOS Memory Pool"/>
        <file category="source" attr="template" name="CMSIS_RTX\UserCodeTemplates\MsgQueue.c"  select="CMSIS-RTOS Message Queue"/>
        <file category="source" attr="template" name="CMSIS_RTX\UserCodeTemplates\Mutex.c"     select="CMSIS-RTOS Mutex"/>
        <file category="source" attr="template" name="CMSIS_RTX\UserCodeTemplates\Semaphore.c" select="CMSIS-RTOS Semaphore"/>
        <file category="source" attr="template" name="CMSIS_RTX\UserCodeTemplates\Thread.c"    select="CMSIS-RTOS Thread"/>
        <file category="source" attr="template" name="CMSIS_RTX\UserCodeTemplates\Timer.c"     select="CMSIS-RTOS Timer"/>
        <!-- tool-chain specific template file -->
        <file category="source" attr="template" condition="ARMCC" name="CMSIS_RTX\SRC\ARM\SVC_Table.s" select="CMSIS-RTOS User SVC"/>
        <file category="source" attr="template" condition="GCC"   name="CMSIS_RTX\SRC\GCC\SVC_Table.S" select="CMSIS-RTOS User SVC"/>
        <file category="source" attr="template" condition="IAR"   name="CMSIS_RTX\SRC\IAR\SVC_Table.s" select="CMSIS-RTOS User SVC"/>

        <!-- CPU and Compiler dependent -->
        <!-- ARMCC -->
        <file category="library" condition="CM0_LE_ARMCC"      name="CMSIS_RTX\LIB\ARM\RTX_CM0.lib"      src="CMSIS_RTX\SRC\ARM"/>
        <file category="library" condition="CM0_BE_ARMCC"      name="CMSIS_RTX\LIB\ARM\RTX_CM0_B.lib"    src="CMSIS_RTX\SRC\ARM"/>
        <file category="library" condition="CM3_LE_ARMCC"      name="CMSIS_RTX\LIB\ARM\RTX_CM3.lib"      src="CMSIS_RTX\SRC\ARM"/>
        <file category="library" condition="CM3_BE_ARMCC"      name="CMSIS_RTX\LIB\ARM\RTX_CM3_B.lib"    src="CMSIS_RTX\SRC\ARM"/>
        <file category="library" condition="CM4_LE_ARMCC_STD"  name="CMSIS_RTX\LIB\ARM\RTX_CM3.lib"      src="CMSIS_RTX\SRC\ARM"/>
        <file category="library" condition="CM4_LE_ARMCC_IFX"  name="CMSIS_RTX\LIB\ARM\RTX_CM3_IFX.lib"  src="CMSIS_RTX\SRC\ARM"/>
        <file category="library" condition="CM4_BE_ARMCC"      name="CMSIS_RTX\LIB\ARM\RTX_CM3_B.lib"    src="CMSIS_RTX\SRC\ARM"/>
        <file category="library" condition="CM4F_LE_ARMCC_STD" name="CMSIS_RTX\LIB\ARM\RTX_CM4.lib"      src="CMSIS_RTX\SRC\ARM"/>
        <file category="library" condition="CM4F_LE_ARMCC_IFX" name="CMSIS_RTX\LIB\ARM\RTX_CM4_IFX.lib"  src="CMSIS_RTX\SRC\ARM"/>
        <file category="library" condition="CM4F_BE_ARMCC"     name="CMSIS_RTX\LIB\ARM\RTX_CM4_B.lib"    src="CMSIS_RTX\SRC\ARM"/>
        <file category="library" condition="CM7_LE_ARMCC"      name="CMSIS_RTX\LIB\ARM\RTX_CM3.lib"      src="CMSIS_RTX\SRC\ARM"/>
        <file category="library" condition="CM7_BE_ARMCC"      name="CMSIS_RTX\LIB\ARM\RTX_CM3_B.lib"    src="CMSIS_RTX\SRC\ARM"/>
        <file category="library" condition="CM7F_LE_ARMCC"     name="CMSIS_RTX\LIB\ARM\RTX_CM4.lib"      src="CMSIS_RTX\SRC\ARM"/>
        <file category="library" condition="CM7F_BE_ARMCC"     name="CMSIS_RTX\LIB\ARM\RTX_CM4_B.lib"    src="CMSIS_RTX\SRC\ARM"/>
        <!-- GCC -->
        <file category="library" condition="CM0_LE_GCC"        name="CMSIS_RTX\LIB\GCC\libRTX_CM0.a"     src="CMSIS_RTX\SRC\GCC"/>
        <file category="library" condition="CM0_BE_GCC"        name="CMSIS_RTX\LIB\GCC\libRTX_CM0_B.a"   src="CMSIS_RTX\SRC\GCC"/>
        <file category="library" condition="CM3_LE_GCC"        name="CMSIS_RTX\LIB\GCC\libRTX_CM3.a"     src="CMSIS_RTX\SRC\GCC"/>
        <file category="library" condition="CM3_BE_GCC"        name="CMSIS_RTX\LIB\GCC\libRTX_CM3_B.a"   src="CMSIS_RTX\SRC\GCC"/>
        <file category="library" condition="CM4_LE_GCC_STD"    name="CMSIS_RTX\LIB\GCC\libRTX_CM3.a"     src="CMSIS_RTX\SRC\GCC"/>
        <file category="library" condition="CM4_LE_GCC_IFX"    name="CMSIS_RTX\LIB\GCC\libRTX_CM3_IFX.a" src="CMSIS_RTX\SRC\GCC"/>
        <file category="library" condition="CM4_BE_GCC"        name="CMSIS_RTX\LIB\GCC\libRTX_CM3_B.a"   src="CMSIS_RTX\SRC\GCC"/>
        <file category="library" condition="CM4F_LE_GCC_STD"   name="CMSIS_RTX\LIB\GCC\libRTX_CM4.a"     src="CMSIS_RTX\SRC\GCC"/>
        <file category="library" condition="CM4F_LE_GCC_IFX"   name="CMSIS_RTX\LIB\GCC\libRTX_CM4_IFX.a" src="CMSIS_RTX\SRC\GCC"/>
        <file category="library" condition="CM4F_BE_GCC"       name="CMSIS_RTX\LIB\GCC\libRTX_CM4_B.a"   src="CMSIS_RTX\SRC\GCC"/>
        <file category="library" condition="CM7_LE_GCC"        name="CMSIS_RTX\LIB\GCC\libRTX_CM3.a"     src="CMSIS_RTX\SRC\GCC"/>
        <file category="library" condition="CM7_BE_GCC"        name="CMSIS_RTX\LIB\GCC\libRTX_CM3_B.a"   src="CMSIS_RTX\SRC\GCC"/>
        <file category="library" condition="CM7F_LE_GCC"       name="CMSIS_RTX\LIB\GCC\libRTX_CM4.a"     src="CMSIS_RTX\SRC\GCC"/>
        <file category="library" condition="CM7F_BE_GCC"       name="CMSIS_RTX\LIB\GCC\libRTX_CM4_B.a"   src="CMSIS_RTX\SRC\GCC"/>
        <!-- IAR -->
        <file category="library" condition="CM0_LE_IAR"        name="CMSIS_RTX\LIB\IAR\RTX_CM0.a"        src="CMSIS_RTX\SRC\IAR"/>
        <file category="library" condition="CM0_BE_IAR"        name="CMSIS_RTX\LIB\IAR\RTX_CM0_B.a"      src="CMSIS_RTX\SRC\IAR"/>
        <file category="library" condition="CM3_LE_IAR"        name="CMSIS_RTX\LIB\IAR\RTX_CM3.a"        src="CMSIS_RTX\SRC\IAR"/>
        <file category="library" condition="CM3_BE_IAR"        name="CMSIS_RTX\LIB\IAR\RTX_CM3_B.a"      src="CMSIS_RTX\SRC\IAR"/>
        <file category="library" condition="CM4_LE_IAR"        name="CMSIS_RTX\LIB\IAR\RTX_CM3.a"        src="CMSIS_RTX\SRC\IAR"/>
        <file category="library" condition="CM4_BE_IAR"        name="CMSIS_RTX\LIB\IAR\RTX_CM3_B.a"      src="CMSIS_RTX\SRC\IAR"/>
        <file category="library" condition="CM4F_LE_IAR"       name="CMSIS_RTX\LIB\IAR\RTX_CM4.a"        src="CMSIS_RTX\SRC\IAR"/>
        <file category="library" condition="CM4F_BE_IAR"       name="CMSIS_RTX\LIB\IAR\RTX_CM4_B.a"      src="CMSIS_RTX\SRC\IAR"/>
        <file category="library" condition="CM7_LE_IAR"        name="CMSIS_RTX\LIB\IAR\RTX_CM3.a"        src="CMSIS_RTX\SRC\IAR"/>
        <file category="library" condition="CM7_BE_IAR"        name="CMSIS_RTX\LIB\IAR\RTX_CM3_B.a"      src="CMSIS_RTX\SRC\IAR"/>
        <file category="library" condition="CM7F_LE_IAR"       name="CMSIS_RTX\LIB\IAR\RTX_CM4.a"        src="CMSIS_RTX\SRC\IAR"/>
        <file category="library" condition="CM7F_BE_IAR"       name="CMSIS_RTX\LIB\IAR\RTX_CM4_B.a"      src="CMSIS_RTX\SRC\IAR"/>
      </files>
    </component>
  </components>
 
  <boards>
    <board name="uVision Simulator" vendor="Keil">
      <description>uVision Simulator</description>
      <mountedDevice    deviceIndex="0" Dvendor="ARM:82" Dname="ARMCM0"/>
      <compatibleDevice deviceIndex="0" Dvendor="ARM:82" Dname="ARMCM3"/>
      <compatibleDevice deviceIndex="0" Dvendor="ARM:82" Dname="ARMCM4_FP"/>
      <compatibleDevice deviceIndex="0" Dvendor="ARM:82" Dname="ARMCM7_DP"/>
    </board>
  </boards>

  <examples>
    <example name="DSP_Lib Class Marks example" doc="Abstract.txt" folder="CMSIS\DSP_Lib\Examples\arm_class_marks_example\ARM">
      <description>DSP_Lib Class Marks example</description>
      <board name="uVision Simulator" vendor="Keil"/>
      <project>
        <environment name="uv" load="arm_class_marks_example.uvprojx"/>
      </project>
      <attributes>
        <component Cclass="CMSIS" Cgroup="CORE"/>
        <component Cclass="CMSIS" Cgroup="DSP"/>
        <component Cclass="Device" Cgroup="Startup"/>
        <category>Getting Started</category>
      </attributes>
    </example>

    <example name="DSP_Lib Convolution example" doc="Abstract.txt" folder="CMSIS\DSP_Lib\Examples\arm_convolution_example\ARM">
      <description>DSP_Lib Convolution example</description>
      <board name="uVision Simulator" vendor="Keil"/>
      <project>
        <environment name="uv" load="arm_convolution_example.uvprojx"/>
      </project>
      <attributes>
        <component Cclass="CMSIS" Cgroup="CORE"/>
        <component Cclass="CMSIS" Cgroup="DSP"/>
        <component Cclass="Device" Cgroup="Startup"/>
        <category>Getting Started</category>
      </attributes>
    </example>

    <example name="DSP_Lib Dotproduct example" doc="Abstract.txt" folder="CMSIS\DSP_Lib\Examples\arm_dotproduct_example\ARM">
      <description>DSP_Lib Dotproduct example</description>
      <board name="uVision Simulator" vendor="Keil"/>
      <project>
        <environment name="uv" load="arm_dotproduct_example.uvprojx"/>
      </project>
      <attributes>
        <component Cclass="CMSIS" Cgroup="CORE"/>
        <component Cclass="CMSIS" Cgroup="DSP"/>
        <component Cclass="Device" Cgroup="Startup"/>
        <category>Getting Started</category>
      </attributes>
    </example>

    <example name="DSP_Lib FFT Bin example" doc="Abstract.txt" folder="CMSIS\DSP_Lib\Examples\arm_fft_bin_example\ARM">
      <description>DSP_Lib FFT Bin example</description>
      <board name="uVision Simulator" vendor="Keil"/>
      <project>
        <environment name="uv" load="arm_fft_bin_example.uvprojx"/>
      </project>
      <attributes>
        <component Cclass="CMSIS" Cgroup="CORE"/>
        <component Cclass="CMSIS" Cgroup="DSP"/>
        <component Cclass="Device" Cgroup="Startup"/>
        <category>Getting Started</category>
      </attributes>
    </example>

    <example name="DSP_Lib FIR example" doc="Abstract.txt" folder="CMSIS\DSP_Lib\Examples\arm_fir_example\ARM">
      <description>DSP_Lib FIR example</description>
      <board name="uVision Simulator" vendor="Keil"/>
      <project>
        <environment name="uv" load="arm_fir_example.uvprojx"/>
      </project>
      <attributes>
        <component Cclass="CMSIS" Cgroup="CORE"/>
        <component Cclass="CMSIS" Cgroup="DSP"/>
        <component Cclass="Device" Cgroup="Startup"/>
        <category>Getting Started</category>
      </attributes>
    </example>

    <example name="DSP_Lib Graphic Equalizer example" doc="Abstract.txt" folder="CMSIS\DSP_Lib\Examples\arm_graphic_equalizer_example\ARM">
      <description>DSP_Lib Graphic Equalizer example</description>
      <board name="uVision Simulator" vendor="Keil"/>
      <project>
        <environment name="uv" load="arm_graphic_equalizer_example.uvprojx"/>
      </project>
      <attributes>
        <component Cclass="CMSIS" Cgroup="CORE"/>
        <component Cclass="CMSIS" Cgroup="DSP"/>
        <component Cclass="Device" Cgroup="Startup"/>
        <category>Getting Started</category>
      </attributes>
    </example>

    <example name="DSP_Lib Linear Interpolation example" doc="Abstract.txt" folder="CMSIS\DSP_Lib\Examples\arm_linear_interp_example\ARM">
      <description>DSP_Lib Linear Interpolation example</description>
      <board name="uVision Simulator" vendor="Keil"/>
      <project>
        <environment name="uv" load="arm_linear_interp_example.uvprojx"/>
      </project>
      <attributes>
        <component Cclass="CMSIS" Cgroup="CORE"/>
        <component Cclass="CMSIS" Cgroup="DSP"/>
        <component Cclass="Device" Cgroup="Startup"/>
        <category>Getting Started</category>
      </attributes>
    </example>

    <example name="DSP_Lib Matrix example" doc="Abstract.txt" folder="CMSIS\DSP_Lib\Examples\arm_matrix_example\ARM">
      <description>DSP_Lib Matrix example</description>
      <board name="uVision Simulator" vendor="Keil"/>
      <project>
        <environment name="uv" load="arm_matrix_example.uvprojx"/>
      </project>
      <attributes>
        <component Cclass="CMSIS" Cgroup="CORE"/>
        <component Cclass="CMSIS" Cgroup="DSP"/>
        <component Cclass="Device" Cgroup="Startup"/>
        <category>Getting Started</category>
      </attributes>
    </example>

    <example name="DSP_Lib Signal Convergence example" doc="Abstract.txt" folder="CMSIS\DSP_Lib\Examples\arm_signal_converge_example\ARM">
      <description>DSP_Lib Signal Convergence example</description>
      <board name="uVision Simulator" vendor="Keil"/>
      <project>
        <environment name="uv" load="arm_signal_converge_example.uvprojx"/>
      </project>
      <attributes>
        <component Cclass="CMSIS" Cgroup="CORE"/>
        <component Cclass="CMSIS" Cgroup="DSP"/>
        <component Cclass="Device" Cgroup="Startup"/>
        <category>Getting Started</category>
      </attributes>
    </example>

    <example name="DSP_Lib Sinus/Cosinus example" doc="Abstract.txt" folder="CMSIS\DSP_Lib\Examples\arm_sin_cos_example\ARM">
      <description>DSP_Lib Sinus/Cosinus example</description>
      <board name="uVision Simulator" vendor="Keil"/>
      <project>
        <environment name="uv" load="arm_sin_cos_example.uvprojx"/>
      </project>
      <attributes>
        <component Cclass="CMSIS" Cgroup="CORE"/>
        <component Cclass="CMSIS" Cgroup="DSP"/>
        <component Cclass="Device" Cgroup="Startup"/>
        <category>Getting Started</category>
      </attributes>
    </example>


    <example name="DSP_Lib Variance example" doc="Abstract.txt" folder="CMSIS\DSP_Lib\Examples\arm_variance_example\ARM">
      <description>DSP_Lib Variance example</description>
      <board name="uVision Simulator" vendor="Keil"/>
      <project>
        <environment name="uv" load="arm_variance_example.uvprojx"/>
      </project>
      <attributes>
        <component Cclass="CMSIS" Cgroup="CORE"/>
        <component Cclass="CMSIS" Cgroup="DSP"/>
        <component Cclass="Device" Cgroup="Startup"/>
        <category>Getting Started</category>
      </attributes>
    </example>
  </examples>

</package>
