/**
 * \file
 *
 * \brief Linker script for running in internal FLASH on the SAMD21E16CU
 *
 * Copyright (c) 2017 Atmel Corporation,
 *                    a wholly owned subsidiary of Microchip Technology Inc.
 *
 * \asf_license_start
 *
 * \page License
 *
 * Licensed under the Apache License, Version 2.0 (the "License");
 * you may not use this file except in compliance with the License.
 * You may obtain a copy of the Licence at
 *
 *     http://www.apache.org/licenses/LICENSE-2.0
 *
 * Unless required by applicable law or agreed to in writing, software
 * distributed under the License is distributed on an "AS IS" BASIS,
 * WITHOUT WARRANTIES OR CONDITIONS OF ANY KIND, either express or implied.
 * See the License for the specific language governing permissions and
 * limitations under the License.
 *
 * \asf_license_stop
 *
 */

/*###ICF### Section handled by ICF editor, don't touch! ****/
/*-Editor annotation file-*/
/* IcfEditorFile="$TOOLKIT_DIR$\config\ide\IcfEditor\cortex_v1_0.xml" */
/*-Specials-*/
define symbol __ICFEDIT_intvec_start__        = 0x00000000;
/*-Memory Regions-*/
define symbol __ICFEDIT_region_RAM_start__    = 0x20000000;
define symbol __ICFEDIT_region_RAM_end__      = 0x20001FFF;
define symbol __ICFEDIT_region_ROM_start__    = 0x00000000;
define symbol __ICFEDIT_region_ROM_end__      = 0x0000FFFF;
/*-Sizes-*/
if (!isdefinedsymbol(__ICFEDIT_size_cstack__)) {
  define symbol __ICFEDIT_size_cstack__    = 0x800;
}
if (!isdefinedsymbol(__ICFEDIT_size_heap__)) {
  define symbol __ICFEDIT_size_heap__      = 0x0;
}
/**** End of ICF editor section. ###ICF###*/

define memory mem with size = 4G;
define region RAM_region    = mem:[from __ICFEDIT_region_RAM_start__ to __ICFEDIT_region_RAM_end__];
define region ROM_region    = mem:[from __ICFEDIT_region_ROM_start__ to __ICFEDIT_region_ROM_end__];

define block CSTACK with alignment = 8, size = __ICFEDIT_size_cstack__ { };
define block HEAP   with alignment = 8, size = __ICFEDIT_size_heap__   { };

initialize by copy  { readwrite };
do not initialize   { section .noinit };

place at address mem:__ICFEDIT_intvec_start__ { readonly section .intvec };
place in ROM_region                           { readonly };
place in RAM_region                           { readwrite };
place at end of RAM_region                    { block CSTACK, block HEAP };
